**Appearance & Interface Description**



* 1. Multi-Function Button
	2. Volume –
	3. Power Button
	4. Volume + (Next Track)
	5. Power Input
	6. TF Card Slot
	7. LED Indicator
	8. AUX-In Port
	9. USB Media Input

**Operation Instructions**

1. **Turning Boom-10 On/Off**

Press and hold the power button to turn on/off the speaker.

1. **Pairing Boom-10**
* The speaker enters Bluetooth mode automatically when turned on.
* Turn on the Bluetooth function of the device you wish to connect and search for “Promate Boom-10”. From the list of found devices, select “Promate Boom-10”.
* Boom-10 will pair automatically with the last connected device.
1. **Using TWS Function**
	* Turn on both speakers and ensure they are in Bluetooth mode.
	* Long press the Multi-Function button on both speakers until you hear a tone.
	* You will hear a tone once both speakers to pair with each other.
	* Once paired, you may pair your device to the speakers using the above-mentioned steps.
2. **USB & TF Card Function**
* Insert the USB media device or TF card into the USB port or TF Card Slot.
* Boom-10 will automatically start playing music files from the USB port or TF Card Slot.
* Control music playback using the Volume Buttons.
1. **Controlling Music Playback**
* **Music Play/Pause:** Press the multi-function button once to play/pause music tracks
* **Music Track Control:** Short press the Volume + or Volume – buttons to skip to the next or previous track.
* **Volume Control:** Long press the Volume + or Volume – buttons to increase or decrease the volume.
1. **AUX Function**
* Connect your playback device via the AUX port to Boom-10.
* Press the Multifunction Button to enter AUX mode.

**Troubleshooting**

1. Boom-10 does not pair with a Bluetooth device:
* Check if the Bluetooth hardware on your device supports A2DP profile which is necessary for sound transmission over Bluetooth.